*
... 

Cmd:  AT

PUH⸮
Cmd:  AT


AT


busy p...

OK

Cmd:  AT+CIPMUX=0

AT+CIPMUX=0

OK

Cmd:  ATE0

ATE0

OK
Init!

Cmd:  AT+CWJAP_CUR="Summ_summ","*******"

WIFI CONNECTED
WIFI GOT IP

OK
WLAN !

Cmd:  AT+SLEEP=0


OK

Cmd:  AT+CIPSTART="TCP","testsystem.beelogger.de",80

CONNECT
Cmd:  AT+CIPSENDEX=300



OK
>GET /rudolf_bee/beelogger6/beelogger_log.php?Passwort=*****&TempIn=22.75&TempOut=20.69&FeuchteIn=999.99&FeuchteOut=999.99&Licht=1015.55&Gewicht=2712&VBatt=12.38&VSolar=12.38&Check=5796.00 HTTP/1.1
Host: testsystem.beelogger.de
Connection: close


Cmd:  AT+CWQAP


OK

Cmd:  AT+RST

WIFI DISCONNECT

OK
